Measurement script:

RECORDDILUTION 0

SETVISCOSITY WATER

CAMERASETTINGSMSG

SYRINGELOAD 1000

DELAY 5

SYRINGELOAD 25

DELAY 10

REPEATSTART

CAPTURE 60

DELAY 1

REPEAT 4

SYRINGESTOP

PROCESSSINGLESETTING

EXPORTRESULTS