|  |  |
| --- | --- |
|  |  |
|   | **Color** | **Wavelength range (nm)** |  |
|   | Infrared | 700 < *λ* < 1200 |  |
|   | [Red](https://en.wikipedia.org/wiki/Red) | 620 < *λ* < 645 |  |
|   | [Red-orange](https://en.wikipedia.org/wiki/Red-orange) | 610 < *λ* < 620 |  |
|   | [Green](https://en.wikipedia.org/wiki/Green) | 520 < *λ* < 550 |  |
|   | [Cyan](https://en.wikipedia.org/wiki/Cyan) | 490 < *λ* < 520 |  |
|   | [Blue](https://en.wikipedia.org/wiki/Blue) | 460 < *λ* < 490 |  |
|   | [Ultraviolet](https://en.wikipedia.org/wiki/Red) | 100 < *λ* < 400 |  |
|  |  |  |  |
|  |  |  |  |